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Автоматически созданное описание]                       TARBOC RH-FY19A
1、 [image: ]Display panel and key definition







Menu key: enter/return to the main menu.
Up key: menu function up selection/parameter increment.
Down key: menu function down selection/parameter decreasing.
Enter key: select the menu function, and confirm and save it when the menu function parameters are modified.
Second, the menu function
After the machine is powered on and reset, press the menu key to enter the main menu (exit after 30 seconds of no operation in the main menu interface). See the main menu menu (5 main menu options in total) for details. Press the Up or Down key to select the main menu, enter the Enter key to modify the function parameters of each menu, and then press the Enter key to save the current function parameters after modification (with power-off memory after saving).
	primary menu
	submenu
	Menu function description

	1. System Settings
	1. DMX address
	Modify the DMX address code up or down (the optional range of address code is 001-512), and press the Enter key to save. The default value is 001.

	
	2. Encoder
	Modify the encoder on/off up or down, save the confirmation key and turn it on by default.

	
	3. X inversion
	Modify the X-reversal on/off up or down, and confirm to save, which is closed by default.

	
	4. Y inversion
	Modify Y-turn on/off up or down, and confirm to save, which is closed by default.

	
	5. Advanced Settings
	

	2. Operation mode
	1. Operation mode
	Select the running mode DMX/ Voice Control/Auto up or down, and press the Enter key to save. The default DMX is selected.

	
	2. Channel selection
	Select channels CH22, CH23, CH25, CH36, CH78, CH92, CH97, CH99 and CH101 up or down, and confirm to save. The default is CH25.

	3. Manual control

	1、X
	Modify the operating parameter value of X motor up or down (adjustable range 000-255), and press the Enter key to save. The default value is 000.

	
	2, X fine tuning
	Modify the fine-tuning parameter value of X motor up or down (adjustable range 000-255), and press the Enter key to save. The default value is 000.

	
	3、Y
	Modify the operating parameter value of Y motor up or down (adjustable range: 000-255), and press the Enter key to save; the default value is 128.

	
	4, y fine-tuning
	Modify the fine-tuning parameter value of Y motor up or down (adjustable range: 000-255), and press the Enter key to save; the default value is 000.

	
	5, XY speed
	Modify the operating speed parameter value of XY motor up or down (adjustable range: 000-255), and press the Enter key to save; the default value is 000.

	
	6, focusing
	Modify the operation parameter value of the focusing motor up or down (adjustable range 000-255), and press the Enter key to save, and the default value is 000.

	
	7. Turn the mirror
	Modify the parameter value of the rotating mirror up or down (adjustable range 000-255), and press OK to save. The default value is 000.

	
	8. Dimming
	Modify the dimming parameter value up or down (adjustable range: 000-255), and press the Enter key to save; the default value is 255.

	
	9, stroboscopic
	Modify the strobe parameter value up or down (adjustable range 000-255), and press the Enter key to save. The default value is 000.

	
	10. The foreground is red
	Modify the red current value up or down (adjustable range: 000-255), and press the Enter key to save; the default value is 255.

	
	11. The foreground is green
	Modify the green current value up or down (adjustable range: 000-255), and press the Enter key to save; the default value is 255.

	
	12. The foreground is blue
	Modify the blue current value up or down (adjustable range: 000-255), and press the Enter key to save; the default value is 255.

	
	13. The foreground is white
	Modify the white current value up or down (adjustable range: 000-255), and press the Enter key to save; the default value is 255.

	
	14. Color temperature
	Modify the color temperature up or down (adjustable range 000-255), and press OK to save. The default value is 000.

	
	15. Dyeing
	Modify the color dyeing value up or down (adjustable range: 000-255), and press the Enter key to save; the default value is 000.

	
	16, desalination
	Modify the color fade value up or down (adjustable range: 000-255), and press OK to save; the default value is 000.

	
	17. Translation
	Modify the translation value up or down (adjustable range: 000-255), and press the Enter key to save; the default value is 000.

	
	18. Patterns
	Modify the color dyeing value up or down (adjustable range: 000-255), and press the Enter key to save; the default value is 000.

	
	19. Moving pictures
	Modify the color animation up or down (adjustable range: 000-255), and press the Enter key to save; the default value is 000.

	
	20. Speed
	Modify the speed up or down (adjustable range 000-255), and press the Enter key to save. The default value is 000.

	
	21. The background color is red
	Modify the red current value up or down (adjustable range: 000-255), and press the Enter key to save; the default value is 000.

	
	22. The background color is green
	Modify the green current value up or down (adjustable range 000-255), and press the Enter key to save. The default value is 000.

	
	23. The background color is blue
	Modify the blue current value up or down (adjustable range: 000-255), and press the Enter key to save; the default value is 000.

	
	24, the background color is white
	Modify the white current value up or down (adjustable range 000-255), and press the Enter key to save. The default value is 000.

	
	25, reset
	When the parameter value is 150-255, the whole machine is reset. The parameter value of the console must be pulled below 10 before it is pushed to 150-255. The parameter value is useless when it is 000-149, so it cannot be reset.

	4. Display settings
	1. Language choice
	Select Chinese /EN (English) up or down, and press the Enter key to save. The default is Chinese.

	
	2. Inverted display settings
	Select up or down to turn off/on the reverse display setting, and press the Enter key to save, which is turned off by default.

	
	3, screen saver settings,
	Select the close/open screen saver setting up or down, and confirm to save it, which is turned on by default.

	
	4. Software version
	06MC

	5. Information
	Encryption settings
	close

	
	time
	9999:00

	
	HALL
	0000110

	6. Factory Settings
	Please enter the password for display! Change it to 138 up or down, and then press the Enter key to enter the factory settings.
	1. X axis calibration
	Modify the parameter up or down (range 000-255), and confirm to save it. The default value is 128.

	
	
	2, Y axis calibration
	Modify the parameter up or down (range 000-255), and confirm to save it. The default value is 128.

	
	
	3, focusing calibration
	Modify the parameter up or down (range 000-255), and confirm to save it. The default value is 128.

	
	
	4, focusing stroke
	Modify the parameter up or down (range 000-255), and press the Enter key to save. The default value is 128.

	
	
	5, rotary calibration
	Modify the parameter up or down (range 000-255), and confirm to save it. The default value is 128.

	
	
	6. Red
	Modify the red light bulb current (032-255) up or down, and press the Enter key to save. The default value is 252.

	
	
	7. Green
	Modify the green light bulb current up or down (032-255), and press the Enter key to save. The default value is 252.

	
	
	8. Blue
	Modify the blue light bulb current up or down (032-255), and press the Enter key to save. The default value is 252.

	
	
	9. White
	Modify the white light bulb current up or down (032-255), and press the Enter key to save. The default value is 252.

	
	
	10. Current
	Select 000 /007 up or down, and confirm to save. The default value is 004.

	
	
	11. Speed
	Modify the speed parameter (range 001-007) up or down, and press OK to save. The default value is 000.

	
	
	12、Logo
	Select 000 /001 up or down, and confirm to save. The default value is 000.

	
	
	13. Temperature
	Modify the temperature parameter (range 045-075) up or down, and confirm to save it. The default value is 065.

	
	
	14. Temperature-Fan
	Select up or down to turn off/on the fan control, and press the Enter key to save, which will be turned off by default.

	
	
	15、LED
	LED-A/LED-B



Third, master-slave control
There are two or more identical lamps connected by DMX three-core signal lines, all lamps are modified to any address code of 001~512, and any one is set as the master, while other lamps are slaves, and all slave displays do not flicker; When the master adjusts the effects of gradual change, pulse change, jump, voice control and self-walking, all slaves synchronize the effects of gradual change, pulse change, jump, voice control and self-walking.
Special attention: 1. Only one host can be set for a group of lamps. If there are multiple hosts, all lamps will flash without synchronization.
2. All lamps and lanterns must be used when the DMX512 console is closed.
Fourth, DMX512 control
Address codes of all lamps and lanterns are set, and all lamps and lanterns are connected to the DMX512 console in parallel with DMX three-core signal lines. The address code stops flashing, indicating that the DMX512 console signal has been sent to the lamps and lanterns. According to the channel description, the DMX512 console is used to control related functions.
CH22 channel description:
	passage
	Channel value
	fundamental function

	one
	000-255
	red

	2
	000-255
	Red fine tuning

	three
	000-255
	green

	four
	000-255
	Green fine tuning

	five
	000-255
	blue

	six
	000-255
	Blue fine tuning

	seven
	000-255
	white

	eight
	000-255
	White fine tuning

	nine
	000-255
	Linear color temperature

	10
	000-255
	Macro function

	11
	000-255
	stroboscopic

	12
	000-255
	Total dimming

	13
	000-255
	Dimming and fine tuning

	14
	000-255
	level

	15
	000-255
	Horizontal fine adjustment

	16
	000-255
	perpendicular/vertical

	17
	000-255
	Vertical fine tuning

	18
	000-255
	function

	19
	000-255
	Reset: The whole machine is reset when the parameter value is between 250 and 255. The console parameter value must be pulled below 10 before it is pushed to 250-255. The parameter value between 000 and 249 is useless and cannot be reset.

	20
	000-255
	focus

	21
	000-255
	rotate

	22
	000-255
	empty



CH23 channel description:
	passage
	Channel value
	fundamental function

	one
	000-255
	X axis

	2
	000-255
	X-axis fine tuning

	three
	000-255
	Y axis

	four
	000-255
	Y axis fine tuning

	five
	000-255
	XY speed

	six
	000-255
	focus

	seven
	000-255
	rotate

	eight
	000-255
	Total dimming

	nine
	000-255
	stroboscopic

	10
	000-255
	glow

	11
	000-255
	green light

	12
	000-255
	blue light

	13
	000-255
	white light

	14
	000-255
	colour temperature

	15
	000-255
	Dyeing/color macro function

	16
	000-255
	Static effect

	17
	000-255
	Dynamic effect

	18
	000-255
	Dynamic effect speed

	19
	000-255
	Red-background color

	20
	000-255
	Green-background color

	21
	000-255
	Blue light-background color

	22
	000-255
	White light-background color

	23
	000-255
	Reset: when the parameter value is 250-255, the whole machine is reset. The parameter value of the console must be pulled below 10 before it is pushed to 250-255, and it is useless when the parameter value is 000-249, so it cannot be reset.


CH25 channel description:
	passage
	Channel value
	fundamental function

	one
	000-255
	X axis

	2
	000-255
	X-axis fine tuning

	three
	000-255
	Y axis

	four
	000-255
	Y axis fine tuning

	five
	000-255
	XY speed

	six
	000-255
	focus

	seven
	000-255
	rotate

	eight
	000-255
	Total dimming

	nine
	000-255
	stroboscopic

	10
	000-255
	glow

	11
	000-255
	green light

	12
	000-255
	blue light

	13
	000-255
	white light

	14
	000-255
	colour temperature

	15
	000-255
	dye

	16
	000-255
	Pattern fading

	17
	000-255
	Pattern translation

	18
	000-255
	Static effect

	19
	000-255
	Dynamic effect

	20
	000-255
	Dynamic effect speed

	21
	000-255
	Red light-background color

	22
	000-255
	Green-background color

	23
	000-255
	Blue light-background color

	24
	000-255
	White light-background color

	25
	000-255
	Reset: when the parameter value is 250-255, the whole machine is reset. The parameter value of the console must be pulled below 10 before it is pushed to 250-255, and it is useless when the parameter value is 000-249, so it cannot be reset.


CH36 channel description:
	passage
	Channel value
	fundamental function

	one
	000-255
	red

	2
	000-255
	Red fine tuning

	three
	000-255
	green

	four
	000-255
	Green fine tuning

	five
	000-255
	blue

	six
	000-255
	Blue fine tuning

	seven
	000-255
	white

	eight
	000-255
	White fine tuning

	nine
	000-255
	Linear color temperature

	10
	000-255
	Macro function

	11
	000-255
	stroboscopic

	12
	000-255
	Total dimming

	13
	000-255
	Dimming and fine tuning

	14
	000-255
	level

	15
	000-255
	Horizontal fine adjustment

	16
	000-255
	perpendicular/vertical

	17
	000-255
	Vertical fine tuning

	18
	000-255
	function

	19
	000-255
	Reset: The whole machine is reset when the parameter value is between 250 and 255. The console parameter value must be pulled below 10 before it is pushed to 250-255. The parameter value between 000 and 249 is useless and cannot be reset.

	20
	000-255
	focus

	21
	000-255
	rotate

	22
	000-255
	Pattern rotation

	23
	000-255
	Pattern effect speed

	24
	000-255
	Fading of pattern effect

	25
	000-255
	Pattern Effect-Red

	26
	000-255
	Pattern Effect-Green

	27
	000-255
	Pattern Effect-Blue

	28
	000-255
	Pattern effect-white

	29
	000-255
	Pattern dimming

	30
	000-255
	Background dimming

	31
	000-255
	Pattern change

	32
	000-255
	Pattern translation

	33
	000-255
	Foreground flicker (inversion)

	34
	000-255
	Background strobe (inversion)

	35
	000-255
	Background Selection (Inverted)

	36
	000-255
	empty



CH78 channel description:
	passage
	Channel value
	fundamental function

	one
	000-255
	Useless

	2
	000-255
	Useless

	three
	000-255
	Useless

	four
	000-255
	Useless

	five
	000-255
	Useless

	six
	000-255
	Useless

	seven
	000-255
	Useless

	eight
	000-255
	Useless

	nine
	000-255
	Linear color temperature

	10
	000-255
	Macro function

	11
	000-255
	stroboscopic

	12
	000-255
	Total dimming

	13
	000-255
	Dimming and fine tuning

	14
	000-255
	level

	15
	000-255
	Horizontal fine adjustment

	16
	000-255
	perpendicular/vertical

	17
	000-255
	Vertical fine tuning

	18
	000-255
	function

	19
	000-255
	Reset: The whole machine is reset when the parameter value is between 250 and 255. The console parameter value must be pulled below 10 before it is pushed to 250-255. The parameter value between 000 and 249 is useless and cannot be reset.

	20
	000-255
	focus

	21
	000-255
	rotate

	22
	000-255
	Dimming of the first red lamp bead

	23
	000-255
	Dimming of the first green lamp bead

	24
	000-255
	Dimming of the first blue lamp bead

	25
	000-255
	Dimming the second red lamp bead

	26
	000-255
	Dimming the second green lamp bead

	27
	000-255
	Dimming of the second blue lamp bead

	…
	…
	… …


	76
	000-255
	The 19th Red Lamp Bead Dimming

	77
	000-255
	The 19th green light bulb dims the light.

	seventy-eight
	000-255
	The 19th Blue Lamp Bead Dimming


CH92 channel description:
	passage
	Channel value
	fundamental function

	one
	000-255
	Useless

	2
	000-255
	Useless

	three
	000-255
	Useless

	four
	000-255
	Useless

	five
	000-255
	Useless

	six
	000-255
	Useless

	seven
	000-255
	Useless

	eight
	000-255
	Useless

	nine
	000-255
	Linear color temperature

	10
	000-255
	Macro function

	11
	000-255
	stroboscopic

	12
	000-255
	Total dimming

	13
	000-255
	Dimming and fine tuning

	14
	000-255
	level

	15
	000-255
	Horizontal fine adjustment

	16
	000-255
	perpendicular/vertical

	17
	000-255
	Vertical fine tuning

	18
	000-255
	function

	19
	000-255
	Reset: The whole machine is reset when the parameter value is between 250 and 255. The console parameter value must be pulled below 10 before it is pushed to 250-255. The parameter value between 000 and 249 is useless and cannot be reset.

	20
	000-255
	focus

	21
	000-255
	rotate

	22
	000-255
	Pattern rotation

	23
	000-255
	Pattern effect speed

	24
	000-255
	Fading of pattern effect

	25
	000-255
	Pattern Effect-Red

	26
	000-255
	Pattern Effect-Green

	27
	000-255
	Pattern Effect-Blue

	28
	000-255
	Pattern effect-white

	29
	000-255
	Pattern dimming

	30
	000-255
	Background dimming

	31
	000-255
	Pattern change

	32
	000-255
	Pattern translation

	33
	000-255
	Foreground flicker (inversion)

	34
	000-255
	Background strobe (inversion)

	35
	000-255
	Background Selection (Inverted)

	36
	000-255
	Dimming of the first red lamp bead

	37
	000-255
	Dimming of the first green lamp bead

	38
	000-255
	Dimming of the first blue lamp bead

	…
	…
	… …


	90
	000-255
	The 19th Red Lamp Bead Dimming

	91
	000-255
	The 19th green light bulb dims the light.

	92
	000-255
	The 19th Blue Lamp Bead Dimming


CH97 channel description:
	passage
	Channel value
	fundamental function

	one
	000-255
	Useless

	2
	000-255
	Useless

	three
	000-255
	Useless

	four
	000-255
	Useless

	five
	000-255
	Useless

	six
	000-255
	Useless

	seven
	000-255
	Useless

	eight
	000-255
	Useless

	nine
	000-255
	Linear color temperature

	10
	000-255
	Macro function

	11
	000-255
	stroboscopic

	12
	000-255
	Total dimming

	13
	000-255
	Dimming and fine tuning

	14
	000-255
	level

	15
	000-255
	Horizontal fine adjustment

	16
	000-255
	perpendicular/vertical

	17
	000-255
	Vertical fine tuning

	18
	000-255
	function

	19
	000-255
	Reset: The whole machine is reset when the parameter value is between 250 and 255. The console parameter value must be pulled below 10 before it is pushed to 250-255. The parameter value between 000 and 249 is useless and cannot be reset.

	20
	000-255
	focus

	21
	000-255
	rotate

	22
	000-255
	Dimming of the first red lamp bead

	23
	000-255
	Dimming of the first green lamp bead

	24
	000-255
	Dimming of the first blue lamp bead

	25
	000-255
	Dimming of the first white lamp bead

	…
	…
	… …


	94
	000-255
	The 19th Red Lamp Bead Dimming

	95
	000-255
	The 19th green light bulb dims the light.

	96
	000-255
	The 19th Blue Lamp Bead Dimming

	97
	000-255
	The 19th White Lamp Bead Dimming


CH99 channel description:
	passage
	Channel value
	fundamental function

	one
	000-255
	X axis

	2
	000-255
	X-axis fine tuning

	three
	000-255
	Y axis

	four
	000-255
	Y axis fine tuning

	five
	000-255
	XY speed

	six
	000-255
	focus

	seven
	000-255
	rotate

	eight
	000-255
	Total dimming

	nine
	000-255
	stroboscopic

	10
	000-255
	Useless

	11
	000-255
	Useless

	12
	000-255
	Useless

	13
	000-255
	Useless

	14
	000-255
	colour temperature

	15
	000-255
	dye

	16
	000-255
	Static effect

	17
	000-255
	Dynamic effect

	18
	000-255
	Dynamic effect speed

	19
	000-255
	Red light-background color

	20
	000-255
	Green-background color

	21
	000-255
	Blue light-background color

	22
	000-255
	White light-background color

	23
	000-255
	Reset: when the parameter value is 250-255, the whole machine is reset. The parameter value of the console must be pulled below 10 before it is pushed to 250-255, and it is useless when the parameter value is 000-249, so it cannot be reset.

	24
	000-255
	Dimming of the first red lamp bead

	25
	000-255
	Dimming of the first green lamp bead

	26
	000-255
	Dimming of the first blue lamp bead

	27
	000-255
	Dimming of the first white lamp bead

	…
	…
	… …


	96
	000-255
	The 19th Red Lamp Bead Dimming

	97
	000-255
	The 19th green light bulb dims the light.

	98
	000-255
	The 19th Blue Lamp Bead Dimming

	99
	000-255
	The 19th White Lamp Bead Dimming


CH101 channel description:
	passage
	Channel value
	fundamental function

	one
	000-255
	X axis

	2
	000-255
	X-axis fine tuning

	three
	000-255
	Y axis

	four
	000-255
	Y axis fine tuning

	five
	000-255
	XY speed

	six
	000-255
	focus

	seven
	000-255
	rotate

	eight
	000-255
	Total dimming

	nine
	000-255
	stroboscopic

	10
	000-255
	Useless

	11
	000-255
	Useless

	12
	000-255
	Useless

	13
	000-255
	Useless

	14
	000-255
	colour temperature

	15
	000-255
	dye

	16
	000-255
	Pattern fading

	17
	000-255
	Pattern translation

	18
	000-255
	Static effect

	19
	000-255
	Dynamic effect

	20
	000-255
	Dynamic effect speed

	21
	000-255
	Red light-background color

	22
	000-255
	Green-background color

	23
	000-255
	Blue light-background color

	24
	000-255
	White light-background color

	25
	000-255
	Reset: when the parameter value is 250-255, the whole machine is reset. The parameter value of the console must be pulled below 10 before it is pushed to 250-255, and it is useless when the parameter value is 000-249, so it cannot be reset.

	26
	000-255
	Dimming of the first red lamp bead

	27
	000-255
	Dimming of the first green lamp bead

	28
	000-255
	Dimming of the first blue lamp bead

	29
	000-255
	Dimming of the first white lamp bead

	…
	…
	… …


	98
	000-255
	The 19th Red Lamp Bead Dimming

	99
	000-255
	The 19th green light bulb dims the light.

	100
	000-255
	The 19th Blue Lamp Bead Dimming

	101
	000-255
	The 19th White Lamp Bead Dimming




V. Technical parameters:
[bookmark: OLE_LINK5]Voltage: AC100~240V 50/60HZ
Lamp beads: 19 four-in-one LED lamp beads
Control mode: DMX512, self-propelled, master-slave, voice control and RDM function.
Channels: CH22, CH23, CH25, CH36, CH78, CH92, CH97, CH99 and CH101.
Dimming: 32bit 0~100% linear dimming
Features: shaking head+dyeing+focusing+pattern+rotation
Working temperature: -30 ~50℃
Strobe frequency: 1~30HZ
Appearance: metal, black
Connection mode: DMX512 input/output/power input/output.
IP grade: IP20
Size: weight:
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