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           TARBOC RH-Q250GQ


RH-Q250GQ

Beam250W of light
Instruction for use
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Thank you for using our products, is safe and effective use of this product to you, before you use this product, please read this instruction manual carefully complete. This manual contains: the performance of the product is and how to safely install, and use of important information, please properly keep, in order to use as a reference. When installing and using relevant instructions must be strictly observed. 
Operation parameters: 

Power supply: AC100V - 240V         Frequency: 50 hz - 60 hz 

Total power: 200w LED               Fuse: 5 a 

Ballast: electronic ballast             Light bulb power: 200W 

Color temperature: 8000 k 

Average life span: 2000H (light bulb and reflective cup overall package, light efficiency and higher service life) 

Control signal: international standard DMX512            Appearance: high temperature resistant plastic 

Light body color: black               Protection level: IP20                15.3 Net KG 

 Function description: 

1. The international standard control signal: DMX512                   2. The number of tong: 18 ch

3.. The number of motor: a total of 10 mute motor 

4. 650000 touch the TFT color LCD interface, easy operation, interface aesthetics, reverse display interface can be 180 degrees. 

5. The X axis rotate for 540 ℃, the Y axis vertical rotation of 230 ℃, with automatic correction. 

6. X, Y axis can reconcile the micro, running software correction positioning function, high precision. 

7. The dimming: 0-100% linear adjustment. 

8. Stroboscopic: double chip stroboscopic (0.5-9 times/SEC), completely linear dimming and variable stroboscopic speed. 

9. Color wheel: with 13 kinds of color + blank (can create sharp air beam effect) 

10. Pattern wheel: with a 17 fixed pattern piece + blank (let you quickly change the beam shape) 

11. A prism: rotating 8+16+24 prism, can be bi-directional rotation, rotation speed is adjustable, making a richer pattern projection effect 

12. Itemization: soft light effect, the design of soft dream effect. 

13. Focus: adopting the combination of three groups of optical lens effect is much better than the beam of light, usually can reflects the pattern of hid            14. The beam Angle: parallel beam Angle: 0-3.8 

15. Overheating intelligent protection                16. Smart bulb switch control, prolong the service life of the bulb



Connection of DMX512 signal: 

The lamps and lanterns use DMX512 signal control model, the control signal of lamps and lanterns is a parallel relationship, the connection is more than one signal lamps and lanterns, it is best to use double core shielded cables. Connection, all through the lamps and lanterns of lamps and lanterns DMX signal on jack (context) INPUT (INPUT) and OUTPUT (OUTPUT) are connected, connect the line of lamps and lanterns 3 core XLRXL plug terminal must correspond to each other, when the connection signal lamps and lanterns, it is recommended to use DMX signal terminal. Can be avoided, due to electrical noise damage control signal, DMX signal terminal device is a XLR plugs connection between 2 and 3 feet a 120 ohm resistance of 1 w, and connect it on the last stage of lamps and lanterns of the OUTPUT (OUTPUT) jack.                 The initial address code calculation method of lamps and lanterns: 

The starting address code of the current light fixture is equal to (the initial address code of the last light fixture) + (the number of channels of the lamp) : 

1. The initial address code of the first lamp is A001. 

2: the basic channel number of the controller should be greater than or equal to the total number of use channels. 

3. Note: when using any controller, each lamp should have its own initial address code. If the initial address code of the first light lamp is set A001, the number of the luminaire number is 18CH; The starting address of the second light fixture is set to A019. The starting address code of the third light fixture is set to A037; And so on and so forth, (this setting also needs to be determined by different control tables) 

Description of installation of lamps and lanterns: 

This luminaire can be placed horizontally, slanting and hanging upside down, and must pay attention to the installation method when hanging and hanging upside down.      Fixed installation of lamps and lanterns: before the positioning of lamps and lanterns, to ensure the stability of the installation site, when the reverse hanging installation, must ensure that the lamps and lanterns is not tumbled down on the supporting frame and handle with a safety rope through the racks and lamps and lanterns, assist hanging; In order to ensure safety. To prevent fall and slide of lamps and lanterns, lamps and lanterns in the installation and debugging, the ban pedestrians pass, regularly check whether the safety rope appear wear away, whether hook screws loosen, if because hanging installation is not stable, lead to fall all consequences arising from the lamps and lanterns manufacturer does not assume any responsibility. 

Light bulb installation: 

1. When replacing the bulb, remove the plastic shell of the lamphead first.          2. Good quality light bulbs are recommended. 

3. Uncharged installation, remove the bulb.         4. Hand untouchable parts of the bulb.   5. Tighten the screws after replacing the bulb.     6, the light bulb work at high temperature, and gas discharge can not continue to supply the physical characteristics of bubble, must therefore be in every time, when the power is completely cooling ability to operate in about 10 minutes, otherwise it will lead to high voltage discharge, short circuit burn out components on the computer console. 

Safety tips!         To ensure your safe use of lamps, read the following safety tips carefully before using them to avoid unnecessary
breakdowns and injuries. 

1. Non-professional personnel, do not remove the fittings in lamps and lanterns without permission. 

2. AC power supply: check whether the local power supply meets the rated voltage requirement. 

3, the lamps and lanterns is according to the type of electric shock protection design, lamps and lanterns should be used with sufficient power supply system grounding, and lamps and lanterns of the ground wire must be connected to the ground of the power supply system. Do not use insulation damaged power cord, at the same time, do not use the power cord overlap on the other wire. 

4, when the installation location and lamps and lanterns, any point on the surface of lamps and lanterns and any easy to burn the explosive keep minimum distance of 10 meters, 2.5 meters from irradiation distance, please do not install the lamps and lanterns is directly in to burn the material surface. 

5. Ambient temperature used in luminaires: (-10 degrees + 40 degrees), the maximum temperature of the lamp surface is 80 degrees, and the lamps and lanterns should be kept away from the liquid material and wet environment. 

6. Make sure the lamps are well grounded before using the lamps, and do not install and remove any parts. 

7. When installing lamps and lanterns, the fixing screws must be fastened, equipped with safety cables and checked regularly. 

8. The continuous working time of the luminaires should not exceed 10 hours, and the interval time of continuous start of the lamps shall not be less than 10. Otherwise, the bulb should be protected from overheating and cannot be triggered normally. 

9. In the process of use, the lamp should be stopped using lamps in time. 

10. When the bulb reaches the rated service life, it should be replaced in time, or there will be a dangerous explosion. 

11. The rotating part of the lamp and the pasting accessories must be checked regularly and loosened, and the shaking should be strengthened in time to prevent accidents. 

12, lamps and lanterns USES is strong wind cooling, accumulate dirt easily, must be conducted once a month to clean, especially the cooling tuyere, otherwise you'll be in a dust jam, lead to bad heat dissipation, the lamps and lanterns is abnormal. 

Difficult method: 
The following is a list of troubleshooting and processing methods. Other maintenance tasks are handled by professional maintenance personnel. One. Light bulbs 

1.1. Due to improper operation, the bulb has not been completely cooled. The lamp should be cooled for more than 10 minutes, so that the inner bulb of the bulb can be fully restored to normal state, and the power supply can be started again. 

1.2. Check whether the bulb has reached the service life and should replace the new bulb. 

1.3. Check whether the bulb and the bubble line are leaking, shedding or not having good contact. 

1.4. Replace the new point bubbler.              Two. The beam appears dim 

2.1. Check whether the bulb has reached the service life and should replace the new bulb. 

2.2. Check that the optical parts or light bulbs are clean, and the light bulbs and other optical devices are accumulated with dust, and the light bulbs and components should be cleaned and maintained regularly. 

Three. The projected image is blurred 

3.1. Check whether the electron focus channel value is suitable for the current projection distance. 

Computer lights work intermittently       4.1. Check whether the fan is running normally to make it dirty. 

4.2. Check whether the internal temperature control switch is closed.    4.3. Check whether the bulb has reached the service life and should replace the new bulb.     5. Although it glows, the computer lamp no longer accepts controller control 

5.1. Check the initial address code and check the connection of the communication line (1 ground 2 minus 3 positive) 

5.2. Add signal amplifier      5.3. When the bulb was not completely cooled, there was an abnormal start operation, and the instantaneous ultra-high voltage of the bubbler was leaking and the CPU of the circuit board channel chip was burned. 

Six. Computer light cannot be started       6.1. Check whether the insurance on the power input socket is fused 

6.2. Lamps and lanterns are not in contact with the line due to vibration during long distance transportation 

6.3. Check the input power, computer board and other connector devices     7. After self-examination, some functions do not accept controller control    7.1. Check that the function has no power at work, or whether the chip is burned by other high pressure shocks.    8. The X and Y axis in the other data have been restored to 0 in the other data, and abnormal noises have occurred 

8.1. At the time of abnormal qi, the high point bubble voltage leakage caused the burning of X and Y axis photoelectric induction circuit board (light lotus root).     8.2. Restart the computer light according to normal procedures     8.3. Push all the channel values of the controller to 0, remote reset computer lamp.        Maintenance and insurance: 

Shutdown operation: before each off, the bulb first closed 10 minutes ahead of time. Let the cooling fan inside heat when using the lamps and lanterns, fast discharge, it can prolong the lamps and lanterns of accessories, especially the service life of the bulb! In order to ensure the lamps and lanterns can steadily run, should keep it clean, open lamps and lanterns for repair or before maintenance work that make sure the power is disconnected, it is important to keep the lamps and lanterns is clean, clean, clean, please regularly not only keep the maximum brightness output, but also can prolong the service life of lamps and lanterns, it is recommended to use high quality glass cleaner and use a clean soft cloth to clean, use the vacuum cleaner at least half an year is clean inside the lamp. 

After-sales service      Attention! When the lamps and lanterns are out of the factory, they are strictly inspected and the packing is in good condition. Please follow the instructions. The fault of the machine is not covered by the machine. 

1. The company will provide technical advice to customers throughout the lifetime. 

2. If the product failure, need to repair, please show me your product warranty card, and fill in related content. At the same time also hope to customers in a timely manner the problems in the products back to us, convenient for our first time to improve the product. 

3. Besides the luminaires, the following accessories can also be selected:     Attachment: power line: 1, instruction: 1 copy 

The choose and buy a Light bulb (customer request) ,Light hook safety cable (customer selection) 

Software features:      1. LCD 650,000 color touch TFT interface, easy to operate and beautiful interface.

2. Physical buttons and touch are both completely independent and can be used in combination

3. Complete all operations independently with the physical keys        4. Complete all operations independently with touch

5. Use the physical buttons and touch mode to complete all operations         6. Intelligent height

7. For example: check hall, the decoupling error in the reset, and give hints.

8. Reset calibration (zero calibration)       9. X axis, Y axis, color wheel, pattern disk           1. Key instructions:
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The "left" and "right" keys function the same way: return to the previous interface         "Up" and "down" key: select and edit
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"Determine" key (that is, "OK" key) : execute function, begin edit, exit edit              Main interface specification

The following is an example of "modifying DMX address code" to describe the use of keys:

1. If it is not the main interface, press the "left" button (one or more times) to return to the main interface

2. Select the "Settings" button under the "upper" or "lower" keys under the main interface     Press "ok" to enter the "Settings" interface

4. Select the "DMX address" by pressing the "up" key or "under" key under the "setting" interface    Press "ok" to enter edit status

6. Modify the DMXDM address code by pressing "up" or "down" key      Press "ok" to exit edit status

If it's a touch screen, the process is more convenient:    1. Touch the "Settings" button in the main interface to enter the "Settings" interface

2. The same (both physical and touch-based buttons can be used) are the same as the previous 4-7 steps.

3.2. Set the interface 
	passageway 
	function 
	numerical value 
	describe 

	1
	Color plate 
	0 - 4
	White light 

	
	
	5 - 9
	White Light + Color 1 

	
	
	10 - 14
	Color 1 

	
	
	15 - 19
	Color 1 +Color 2

	
	
	20 - 24
	Color 2

	
	
	25 - 29
	Color 2+Color 3

	
	
	30 - 34
	Color3

	
	
	35 - 39
	Color3+Color4

	
	
	40 - 44
	Color4

	
	
	45 - 49
	Color4+Color5

	
	
	50 - 54
	Color5

	
	
	55 - 59
	Color5+Color6

	
	
	60 - 64
	Color6

	
	
	65 - 69
	Color6+Color7

	
	
	70 - 74
	Color7

	
	
	75 - 79
	Color7+Color8

	
	
	80 - 84
	Color8

	
	
	85 - 89
	Color8+Color9

	
	
	90 - 94
	Color9

	
	
	95 - 99
	Color9+Color10

	
	
	100 - 104
	Color10

	
	
	105 - 109
	Color10+Color11

	
	
	110 - 114
	Color11

	
	
	115 - 119
	Color11+Color12

	
	
	120 - 124
	Color12

	
	
	125 - 129
	Color12+Color13

	
	
	130 - 134
	Color13

	
	
	135 - 139
	Color13+白光

	
	
	140 - 197
	Clockwise rotation from fast to slow 

	
	
	198 - 255
	Counter-clockwise rotation from slow to fast 

	2
	Strobe 
	 0 - 3
	Dimming 

	
	
	4 - 55
	Ordinary strobe 

	
	
	56 - 66
	Dimming 

	
	
	67 - 118
	Slow Light Fast Out 

	
	
	119 - 129
	Dimming 

	
	
	130 - 181
	Fast Light Slow Out 

	
	
	182 - 192
	Dimming 

	
	
	193 - 244
	Lightning strobe 

	
	
	245 - 255
	Dimming 

	3
	Dimming 
	0-255
	0-100% Linear Dimming 

	4
	Gutu 
	0 - 4
	round hole 

	
	
	5 - 9
	Pattern 1 

	
	
	10 - 14
	Pattern2

	
	
	15 - 19
	Pattern3

	
	
	20 - 24
	Pattern4

	
	
	25 - 29
	Pattern5

	
	
	30 - 34
	Pattern6

	
	
	35 - 39
	Pattern7

	
	
	40 - 44
	Pattern8

	
	
	45 - 49
	Pattern9

	
	
	50 - 54
	Pattern10

	
	
	55 - 59
	Pattern11

	
	
	60 - 64
	Pattern12

	
	
	65 - 69
	Pattern13

	
	
	70 - 74
	Pattern14

	
	
	75 - 125
	Clockwise rotation from fast to slow 

	
	
	126 - 129
	round hole 

	
	
	130 - 180
	Counter-clockwise rotation from slow to fast 

	
	
	181 - 185
	Round hole dither 

	
	
	186 - 190
	Pattern 1 Jitter 

	
	
	191 - 195
	Pattern 2 Jitter 

	
	
	196 - 200
	Pattern 3 Jitter 

	
	
	201 - 205
	Pattern 4 Jitter 

	
	
	206 - 210
	Pattern 5Jitter 

	
	
	211 - 215
	Pattern 6 Jitter 

	
	
	216 - 220
	Pattern 7 Jitter 

	
	
	221 - 225
	Pattern 8 Jitter 

	
	
	226 - 230
	Pattern 9 Jitter 

	
	
	231 - 235
	Pattern 10 Jitter 

	
	
	236 - 240
	Pattern 11 Jitter 

	
	
	241 - 245
	Pattern 12 Jitter 

	
	
	246 - 250
	Pattern 13Jitter 

	
	
	251 - 255
	Pattern 14 Jitter 

	5
	Prism 
	0 - 127
	No action 

	
	
	128 - 255
	Cut-in prism 

	6
	Prism rotation
	0 - 127
	Linear rotation

	
	
	128 - 189
	Clockwise rotation from fast to slow 

	
	
	189 - 194
	Stop spinning 

	
	
	195 - 255
	Counter-clockwise rotation from slow to fast 

	7
	Atomization
	0 - 127
	No action

	
	
	128 - 255
	Cut atomization 

	8
	Colorful
	0 - 127
	No action

	
	
	128 - 255
	Cutting into the seven colors  

	9
	to focus 
	0-255
	0-100% linear focus 

	10
	X
	0-255
	0-540 degree 

	11
	X Shaft trimming 
	0-255
	X 16bit

	12
	Y
	0-255
	0-270 degree 

	13
	Y Shaft trimming 
	0-255
	Y 16bit

	14
	Macro function 
	0-255
	

	15
	to regain the throne 
	0 - 25
	invalid 

	
	
	26 - 76
	Small motor reset 

	
	
	77 - 127
	XY reset

	
	
	128 - 255
	All reset 

	16
	Head ring total dimming 
	0 - 255
	

	17
	Head strobe  
	0 - 255
	

	18
	Head ring R
	0 - 255
	

	19
	Head ring G
	0 - 255
	

	20
	Head ring B
	0 - 255
	

	21
	Head Circle Effect 
	0 - 255
	

	22
	Head Circle Effect Speed 
	0 - 255
	


 Instruction manual


   Please read the instructions carefully and keep them properly before using the product.
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