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1、 Definition of display panel and key






Menu key: enter/return to the main menu
Up key: menu function select up/parameter increment
Down key: menu function select down/parameter decrement
Confirm key: select the menu function, and confirm and save when modifying the menu function parameters.
II. Menu function
After the machine is powered on and reset, press the menu key to enter the main menu (exit after 30 seconds of no operation on the main menu interface). For details, see the Main Menu Function Table (5 main menu options in total). Press the up or down key to select the main menu, and press the Enter key to modify the function parameters of each menu. After modification, press the Enter key to save the current function parameters (power-off memory is available after saving).
	Main menu
	Submenu
	Menu function description

	1. System settings
	1. DMX address
	Modify the DMX address code up or down (the address code can be selected from 001-512), press the Enter key to save, and the default is 001.

	
	2. Encoder
	Up or down to modify the encoder on/off, the confirmation key to save, the default on.

	
	3. X reversal
	Modify X up or down to reverse on/off, enter to save, off by default.

	
	4. Y reversal
	Modify Y up or down to reverse on/off, enter to save, off by default.

	2. Operation mode
	1. Operation mode
	Up or down to select the operating mode DMX/Voice/Auto, enter to save, default to DMX.

	
	2. Channel selection
	Select the channel CH21 and CH49 up or down, press the OK key to save, and the default is CH21.

	3. Manual control

	1、X
	Modify the running parameter value of X motor upward or downward (the adjustable range is 000-255), press the Enter key to save, and the default value is 000.

	
	2. X fine adjustment
	Modify the X fine tuning parameter value upward or downward (the adjustable range is 000-255), press the Enter key to save, and the default value is 000.

	
	3、Y
	Modify the running parameter value of Y motor upward or downward (adjustable range: 000-255), press Enter to save, and the default value is 128.

	
	3. Y fine adjustment
	Modify the Y fine adjustment parameter value upward or downward (adjustable range: 000-255), press the Enter key to save, and the default is 000.

	
	3. XY speed
	Modify the XY speed parameter value upward or downward (adjustable range: 000-255), press the Enter key to save, and the default value is 000.

	
	3. Dimming
	Modify the dimming parameter value upward or downward (adjustable range: 000-255), press the Enter key to save, and the default value is 255.

	
	4. Strobe
	Modify the stroboscopic parameter value upward or downward (the adjustable range is 000-255), press the Enter key to save, and the default value is 000.

	
	7. Red
	Modify the brightness of the red lamp bead upward or downward (adjustable range: 000-255). Press the Enter key to save. The default value is 255.

	
	8. Green
	Modify the brightness of the green lamp bead upward or downward (adjustable range: 000-255). Press the Enter key to save. The default value is 255.

	
	9. Blue
	Modify the brightness of the blue lamp bead upward or downward (adjustable range: 000-255). Press the Enter key to save. The default value is 255.

	
	10. White
	Modify the brightness of the white lamp bead upward or downward (adjustable range: 000-255), press the confirmation key to save, and the default value is 255.

	
	3. Focus
	Modify the focusing parameter value upward or downward (adjustable range: 000-255), press the Enter key to save, and the default value is 000.

	
	3. Mode
	Modify the mode parameter value upward or downward (the adjustable range is 000-255), press the Enter key to save, and the default is 000.

	
	3. Speed
	Modify the speed parameter value upward or downward (adjustable range: 000-255), press the Enter key to save, and the default value is 000.

	
	3. Color temperature
	Modify the color temperature parameter value upward or downward (adjustable range: 000-255), press the Enter key to save, and the default value is 000.

	
	3. Reset
	Modify the reset parameter value upward or downward (adjustable range: 000-255), press the Enter key to save, and the default value is 000.

	4. Display settings
	1. Language selection
	Select Chinese/EN (English) up or down, and press Enter to save. The default is Chinese.

	
	2. Inverted display settings
	Select up or down to close/open the reverse display setting, and press the confirmation key to save. It is closed by default.

	
	3. Screen saver
	Select up or down to turn off/on the screen saver, and press Enter to save. It is turned on by default.

	
	4. Software version
	03 VA Program Identifier, not modifiable.

	5. Factory settings
	Display, please enter the password! Change up or down to 138, and then press the confirmation key to enter the factory settings.
	1. X-axis calibration
	Modify the parameter up or down (range: 000-255), press the OK key to save, and the default value is 128.

	
	
	2. Y-axis calibration
	Modify the parameter up or down (range: 000-255), press the OK key to save, and the default value is 128.

	
	
	3. Focus calibration
	Modify the parameter up or down (range: 000-255), press the OK key to save, and the default value is 128.

	
	
	4. Rotation calibration
	Modify the parameter up or down (range: 000-255), press the OK key to save, and the default value is 128.

	
	
	5. Red
	Modify the current of the red lamp bead up or down (032-255), press the OK key to save, and the default is 252.

	
	
	6. Green
	Modify the current of the green lamp bead up or down (032-255), press the OK key to save, and the default is 252.

	
	
	7. Blue
	Modify the current of the blue lamp bead (032-255) upward or downward, press the OK key to save, and the default is 252.

	
	
	8. White
	Modify the current of the white lamp bead up or down (032-255), press the OK key to save, and the default is 252.

	
	
	9. Current
	Modify the current up or down (000-007), press the OK key to save, and the default is 004.

	
	
	10. Speed
	Change the speed up or down (032-255), press the OK key to save, and the default is 000.

	
	
	11、Logo
	Select 000/001 up or down and press OK to save. The default value is 000.

	
	
	12. Temperature
	Modify the temperature parameter up or down (range 40-70), press the OK key to save, and the default value is 065.

	
	
	13. Temperature-Fan
	Up or down to select off/on temperature-fan control, enter key to save, default on.



III. Master-slave control
Two or more identical lamps are connected by DMX three-core signal line, all lamps are modified to any address code from 001 to 512, any one is set as the host, other lamps are slave, and the display screen of all slave does not flicker; When the host computer is used to adjust the effects of gradual change, pulse change, jump change, sound control and self-walking, all slave computers shall synchronize the effects of gradual change, pulse change, jump change, sound control and self-walking.
Special note: 1. Only one host can be set for a group of lamps. If there are multiple hosts, all lamps will flash randomly and not be synchronized.
2. All lamps must work only when the DMX512 console is turned off.
IV. DMX512 control
After the address codes of all lamps are set, connect all lamps to the DMX512 console in parallel with the DMX three-core signal line. The address code stops flashing, indicating that the DMX512 console signal has been sent to the lamps. Control relevant functions with the DMX512console according to the channel description.

21 channel description:
	Passageway
	Channel value
	Basic functions

	1
	000-255
	X-axis motor (horizontal direction)

	2
	000-255
	X-axis fine adjustment

	3
	000-255
	Y-axis motor (horizontal direction)

	4
	000-255
	Y Fine adjustment

	5
	000-255
	XY speed

	6
	000-255
	Focus

	7
	000-255
	Rotation

	8
	000-255
	Total dimming

	9
	000-255
	Strobe

	10
	000-255
	Red-Foreground color

	11
	000-255
	Green-Foreground color

	12
	000-255
	Blue-foreground color

	13
	000-255
	White-Foreground Color

	14
	000-255
	Color temperature

	15
	000-255
	Pattern

	16
	000-255
	Speed

	17
	000-255
	Red-background color

	18
	000-255
	Green-background color

	19
	000-255
	Blue-background color

	20
	000-255
	White-background color

	21
	000-255
	Reset: The parameter value is kept at 250-255 for 3 seconds to reset the whole machine. The console parameter value must be pulled below 10 first, and then pushed to 250-255 to be useful. The parameter value has no effect at 000-249 and cannot be reset.


49 Channel Description:
	Passageway
	Channel value
	Basic functions

	1
	000-255
	X-axis motor (horizontal direction)

	2
	000-255
	X-axis fine adjustment

	3
	000-255
	Y-axis motor (horizontal direction)

	4
	000-255
	Y Fine adjustment

	5
	000-255
	XY speed

	6
	000-255
	Focus

	7
	000-255
	Rotation

	8
	000-255
	Total dimming

	9
	000-255
	Strobe

	10
	000-255
	Red-Foreground color

	11
	000-255
	Green-Foreground color

	12
	000-255
	Blue-foreground color

	13
	000-255
	White-Foreground Color

	14
	000-255
	Color temperature

	15
	000-255
	Gif

	16
	000-255
	Gif speed

	17
	000-255
	Red-background color

	18
	000-255
	Green-background color

	19
	000-255
	Blue-background color

	20
	000-255
	White-background color

	21
	000-255
	Reset: The parameter value is kept at 250-255 for 3 seconds to reset the whole machine. The console parameter value must be pulled below 10 first, and then pushed to 250-255 to be useful. The parameter value has no effect at 000-249 and cannot be reset.

	22
	000-255
	The first red light bead

	23
	000-255
	1st green lamp bead

	24
	000-255
	1st blue lamp bead

	25
	000-255
	1st white lamp bead

	…
	… …
	… …

	46
	000-255
	The 7th Red Light Bead

	47
	000-255
	The 7th green lamp bead

	48
	000-255
	7th blue lamp bead

	49
	000-255
	7th white lamp bead



V. Technical parameters
[bookmark: OLE_LINK5]Voltage: AC100 ~ 240V 50/60HZ
Power: 350 W
Lamp beads: 7 4-in-1 LED lamp beads
Control mode: DMX512, self-propelled, master-slave, voice control, with RDM function.
Channels: CH 21, CH 49
Dimming: 32bit 0 ~ 100% linear dimming
Features: head shaking + dyeing + flash + rotation
Working temperature: -30 ℃ ~ 50 ℃
Strobe frequency: 1 ~ 30HZ
Appearance: metal, black
Connection mode: DMX512 input/output/power input/output.
IP rating: IP20
Dimensions: Weight:
2
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