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              TARBOC RH-B19S

1、 Definition of display panel and buttons[image: image1.png]
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Menu key: enter/return to the main menu

Up button: menu function up selection/parameter increment

Down button: menu function down selection/parameter decrease

Confirm key: Select the menu function and make a confirmation and save when modifying the menu function parameters.

二、MENU
After the machine is powered on and reset, press the Menu key to enter the main menu (exit after 30 seconds of no operation on the main menu interface). See the main menu menu for details(5 main menu options in total); Press the up or down keys to select the main menu, confirm the key to enter and modify the functional parameters of each menu, and then press the confirm key to save the current functional parameters (with power down memory after saving).
	Main Menu
	Submenu
	Menu Function Description

	1、System settings
	1. DMA address
	Modify the DMA address code up or down (with an optional range of 001-512), confirm to save, and default to 001.

	
	2. Encoder
	Modify the encoder on/off up or down, save with the confirm button, and default to on.

	
	3. X Invert
	Modify X up or down to reverse on/off, confirm to save, default to off.

	
	4. Y Invert
	Modify Y up or down to reverse on/off, confirm to save, default to off.

	
	5. Advanced Settings
	

	2、Operating mode
	1. Operating mode
	Select the operation mode up or down, such as DMA/voice control/automatic, and press the confirm button to save. The default mode is DMA.

	
	2. Channel selection
	Select channels CH16 and CH24 up or down, confirm to save, default to CH16.

	3、manual

	1. X
	Modify the operating parameter values of X motor up or down (adjustable range 000-255), confirm and save, default to 000.

	
	2. Y
	Modify the operating parameter values of the Y motor up or down (adjustable range 000-255), confirm and save, default to 128.

	
	3. XY speed
	Modify the XY speed parameter value up or down (adjustable range 000-255), confirm to save, default to 000.

	
	4. Dimming
	Modify the dimming parameter values up or down (adjustable range 000-255), confirm to save, default to 255.

	
	5. Red
	Modify the brightness of the red light bead up or down (adjustable range 000-255), confirm to save, default to 255.

	
	6. Green
	Modify the green light bead brightness up or down (adjustable range 000-255), confirm to save, default to 255.

	
	7. Blue
	Modify the brightness of the blue light bead up or down (adjustable range 000-255), confirm to save, default to 255.

	
	8. White
	Modify the brightness of the white light bead up or down (adjustable range 000-255), confirm to save, default to 255.

	
	9. Strobe
	Modify the strobe parameter value up or down (adjustable range 000-255), confirm to save, default to 000.

	
	10. Focusing
	Modify the focusing parameter values up or down (adjustable range 000-255), confirm and save, default to 000.

	
	11. Mode
	Modify the mode parameter values up or down (adjustable range 000-255), confirm to save, default to 000.

	
	12. Speed
	Modify the speed parameter value up or down (adjustable range 000-255), confirm to save, default to 000.

	
	13. X fine tuning
	Modify the operating parameter values of the X fine adjustment motor up or down (adjustable range 000-255), confirm and save, default to 000.

	
	14. Y fine tuning
	Modify the operating parameter values of the Y fine-tuning motor up or down (adjustable range 000-255), confirm and save, default to 000.

	
	15. Reset
	Modify the reset parameter values up or down (adjustable range 000-255), confirm to save, default to 000.

	
	16. Color temperature
	Adjust the color temperature level parameter value up or down (adjustable range 000-255), confirm to save, default to 000.

	4、Display Settings
	1. Language selection
	Select Chinese/EN (English) up or down, confirm to save, default to Chinese.

	
	2. Invert Settings
	Select up or down to turn off/on the inverted display setting, confirm to save, default to off.

	
	3. Screen saver
	Select up or down to turn off/on screen saver, confirm to save, default to on.

	
	4. Software version
	06MC program identification code, cannot be modified.

	4、information
	1. Encryption settings
	close

	
	2. Time
	9999:00

	
	3. HALL
	0000110

	5、Factory settings
	Please enter password for display! Change up or down to 138, and then press the confirm button to enter the factory settings.
	1. X-axis calibration
	Modify the parameters up or down (range 000-255), confirm and save, default to 128.

	
	
	2. Y-axis calibration
	Modify the parameters up or down (range 000-255), confirm and save, default to 128.

	
	
	3. Focusing calibration
	Modify the parameters up or down (range 000-255), confirm and save, default to 128.

	
	
	4. Rotation calibration
	Modify the parameters up or down (range 000-255), confirm and save, default to 128.

	
	
	5. Red
	Modify the red light bead current (032-255) up or down, confirm to save, default to 252.

	
	
	6. Green
	Modify the green light bead current (032-255) up or down, confirm to save, default to 252.

	
	
	7. Blue
	Modify the blue light bead current (032-255) up or down, confirm to save, default to 252.

	
	
	8. White
	Modify the white light bead current (032-255) up or down, confirm to save, default to 252.

	
	
	9. Current
	Modify the current (000-007) up or down, confirm to save, default to 004.

	
	
	10. Speed
	Modify the speed up or down (032-255), confirm to save, default to 000.

	
	
	11. Logo
	Select 000/001 up or down, confirm to save, default to 000.

	
	
	12. Temperature
	Modify the temperature parameters up or down (range 40-70), confirm and save, default to 065.

	
	
	13、Temperature - Fan
	Select up or down to turn off/on temperature fan control, confirm to save, default to on.


三、Master slave control
Two or more identical lighting fixtures are connected with a three core signal wire using a DMA. All lighting fixtures are modified to any address code from 001 to 512, and any one is set as the host, while the other lighting fixtures are set as the slave. All slave display screens do not flash; When using the host to adjust the gradient, pulse, jump, voice control, and self-propelled effects, all slaves synchronize the gradient, pulse, jump, voice control, and self-propelled effects.

Special note: 1. Only one host can be set for a group of lighting fixtures. If there are multiple hosts, all lighting fixtures will flash randomly and not synchronize.

2. All lighting fixtures must be functional when the DMX512 console is turned off.

3. 四、DMX512control
Set the address codes of all lighting fixtures and connect them in parallel with the DMX512 console using a three core signal wire. The address code stops flashing, indicating that the DMX512 console signal has been sent to the lighting fixture. According to the channel instructions, use the DMX512 console to control the relevant functions.

16Channel Description：

	thoroughfare
	channel value
	basic function

	1
	000-255
	X-axis motor (horizontal direction)

	2
	000-255
	Y-axis motor (vertical direction)

	3
	000-255
	XY speed

	4
	000-255
	Total dimming

	5
	000-255
	R

	6
	000-255
	G

	7
	000-255
	B

	8
	000-255
	W

	9
	000-255
	Strobe

	10
	000-255
	focusing

	11
	000-255
	Functional mode

	12
	000-255
	Function mode speed

	13
	000-255
	X fine tuning

	14
	000-255
	Y fine tuning

	15
	000-255
	000-249 invalid 250-255 reset

	16
	000-255
	Color temperature


24Channel Description：

	thoroughfare
	channel value
	basic function

	1
	000-255
	X-axis motor (horizontal direction)

	2
	000-255
	Y-axis motor (vertical direction)

	3
	000-255
	XY speed

	4
	000-255
	Total dimming

	5
	000-255
	R1

	6
	000-255
	G1

	7
	000-255
	B1

	8
	000-255
	W1


	9
	000-255
	R2

	10
	000-255
	G2

	11
	000-255
	B2

	12
	000-255
	W2

	13
	000-255
	R3

	14
	000-255
	G3

	15
	000-255
	B3

	16
	000-255
	W3

	17
	000-255
	Strobe

	18
	000-255
	focusing

	19
	000-255
	Functional mode

	20
	000-255
	Mode speed

	21
	000-255
	X fine tuning

	22
	000-255
	Y fine tuning

	23
	000-255
	000-249 invalid 250-255 reset

	24
	000-255
	Color temperature


五Technical parameters

Voltage: AC100~240V 50/60HZ

Power: 220W

Lamp beads: 19 four in one LED lamp beads

Control mode: DMX512, self-propelled, master-slave, voice control, with RDM function.

Channel: CH16, CH24

Dimming: 32bit 0-100% linear dimming

Features: shaking the head+dyeing+flashing+focusing

Working temperature: -30 ° C~50 ° C

Strobe frequency: 1-30Hz

Appearance: Metal, black

Connection method: DMX512 input/output/power input/output.

IP level: IP20

Size: Weight:
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