[bookmark: Sheet1][bookmark: Sheet2]Rotating retro lamp
1. working voltage: AC220V/50Hz.
2, product power: 250W three 60W golden light
36 3535 three-in-one lamp beads (3W one) and one 40W four-in- one lamp bead
4. Control mode: DMX512, 15 channels, 20 channels and 26 channels.
5. Working mode: DMX512, master/slave, self-propelled, voice contr
6. Dimming mode: 0~100% ultra-smooth dimming.
7. Strobe: 25 times/second

	

	channe
	function
	DMX value
	describe

	1
	X axis
	0-255
	0~360 degrees

	
2
	
X Wuji
	0-49
	0-360 degree rotation (fast to slow) X axis speed e

	
	
	50-152
	Clockwise stepless rotation (from fast to slow)

	
	
	153-255
	Counter-clock stepless rotation (from slow to fast)

	3
	otal dimming of golden ligh
	0-255
	Linear dimming from dark to light

	4
	stroboscopic
	0
	No function

	
	
	1-255
	Synchronous strobe speed from slow to fast (1HZ~25H

	


5
	


Golden light
	0-4
	Extinguish light

	
	
	5-41
	Golden light 1

	
	
	42-76
	Golden light 2

	
	
	77-112
	Golden light 3

	
	
	113-148
	Golden light 1+ golden light 2

	
	
	149-184
	Golden light 2+ golden light 3

	
	
	185-220
	Golden light 2+ golden light 3

	
	
	221-255
	Golden light 1+ golden light 2+ golden light 3

	6
	Dyeing total dimming
	
	Linear dimming from dark to light

	7
	stroboscopic
	0
	

	
	
	1-255
	Synchronous strobe speed from slow to fast (1HZ~25H

	


8
	


1 (dyeing effect running co
	0-4
	Extinguish light

	
	
	5-41
	red

	
	
	42-76
	green

	
	
	77-112
	blue

	
	
	113-148
	Red+green

	
	
	149-184
	Red+blue

	
	
	185-220
	Green+blue


[image: Изображение выглядит как Графика, Шрифт, графический дизайн, логотип

Автоматически созданное описание]                                  TARBOC RH-FG303


2

	
	
	221-255
	Red+Green+Blue

	


9
	


g 2 (base color of dyeing ef
	0-4
	Extinguish light

	
	
	5-41
	red

	
	
	42-76
	green

	
	
	77-112
	blue

	
	
	113-148
	Red+green

	
	
	149-184
	Red+blue

	
	
	185-220
	Green+blue

	
	
	221-255
	Red+Green+Blue

	


10
	


Dyeing 3
	0-4
	Extinguish light

	
	
	5-41
	red

	
	
	42-76
	green

	
	
	77-112
	blue

	
	
	113-148
	Red+green

	
	
	149-184
	Red+blue

	
	
	185-220
	Green+blue

	
	
	221-255
	Red+Green+Blue

	




11
	




beam
	0-4
	Extinguish light

	
	
	5-36
	red

	
	
	37-48
	green

	
	
	48-79
	blue

	
	
	80-111
	white

	
	
	112-144
	Red+green

	
	
	145-176
	Red+blue

	
	
	177-208
	Green+blue

	
	
	209-240
	Red++Green+Blue

	
	
	241-255
	Red++Green+Blue+White

	
12
	
golden light) macro functio
	0-4
	neutrality

	
	
	5-85
86-170
171-255
	Built-in effect 1 (from slow to fast)
Built-in effect 2 (from slow to fast) Built-in effect 3 (from slow to fast)

	
	
	
	

	


13
	


dyeing light) macro functio
	0-4
	neutrality

	
	
	4-45
	Built-in effect 1 (from slow to fast)

	
	
	46-87
	Built-in effect 2 (from slow to fast)

	
	
	88-129
	Built-in effect 3 (from slow to fast)

	
	
	130-171
	Built-in effect 4 (from slow to fast)

	
	
	172-213
	Built-in effect 5 (from slow to fast)

	
	
	213-255
	Built-in effect 6 (from slow to fast)

	
14
	
(beam) macro function
	0-4
	neutrality

	
	
	5-85
86-170
171-255
	Built-in effect 1 (from slow to fast) Built-in effect 2 (from slow to fast) Built-in effect 3 (from slow to fast)

	
	
	
	

	
15	reset
	0-199
200-255
	neutrality reset



	channe
	function
	DMX value
	describe

	1
	X axis
	0-255
	0~360 degrees

	
2
	
X Wuji
	0-49
	0-360 degree rotation (fast to slow) X axis speed e

	
	
	50-152
	Clockwise stepless rotation (from fast to slow)

	
	
	153-255
	Counter-clock stepless rotation (from slow to fast)

	3
	otal dimming of golden ligh
	0-255
	Linear dimming from dark to light

	4
	stroboscopic
	0
	No function

	
	
	1-255
	Synchronous strobe speed from slow to fast (1HZ~25H

	5
	Golden light 1
Golden light 2
Golden light 3 Dyeing total dimming
Dyeing stroboscopic
	0-255
	Linear dimming from dark to light

	6
	
	0-255
	Linear dimming from dark to light

	7
	
	0-255
	Linear dimming from dark to light

	8
	
	0-255
	Linear dimming from dark to light

	9
	
	0
	No function

	
	
	1-255
	Synchronous strobe speed from slow to fast (1HZ~25H

	10
11
12
13
14
15
16
	light (dyeing effect runnin ight (background color of dy Dyed blue light
Beam red light Beam green light Blue light beam
Beam white light
	0-255
	Linear dimming from dark to light

	
	
	0-255
	Linear dimming from dark to light

	
	
	0-255
	Linear dimming from dark to light

	
	
	0-255
	Linear dimming from dark to light

	
	
	0-255
	Linear dimming from dark to light

	
	
	0-255
	Linear dimming from dark to light

	
	
	0-255
	Linear dimming from dark to light

	
17
	
golden light) macro functio
	0-4
	neutrality

	
	
	5-85
86-170
171-255
	Built-in effect 1 (from slow to fast)
Built-in effect 2 (from slow to fast) Built-in effect 3 (from slow to fast)

	
	
	
	

	

18
	

dyeing light) macro functio
	0-4
	neutrality

	
	
	4-45
	Built-in effect 1 (from slow to fast)

	
	
	46-87
	Built-in effect 2 (from slow to fast)

	
	
	88-129
	Built-in effect 3 (from slow to fast)

	
	
	130-171
	Built-in effect 4 (from slow to fast)

	
	
	172-213
	Built-in effect 5 (from slow to fast)

	
	
	213-255
	Built-in effect 6 (from slow to fast)

	
19
	
(beam) macro function
	0-4
	neutrality

	
	
	5-85
86-170
171-255
	Built-in effect 1 (from slow to fast) Built-in effect 2 (from slow to fast)
Built-in effect 3 (from slow to fast)

	
	
	
	

	20	reset
	0-199
200-255
	neutrality
reset



	6 channe
	function
	DMX value
	describe

	1
	X axis
	0-255
	0~360 degrees

	
2
	
X Wuji
	0-49
	0-360 degree rotation (fast to slow) X axis speed e

	
	
	50-152
	Clockwise stepless rotation (from fast to slow)

	
	
	153-255
	Counter-clock stepless rotation (from slow to fast)

	3
	otal dimming of golden ligh
	0-255
	Linear dimming from dark to light

	4
	stroboscopic
	0
	No function

	
	
	1-255
	Synchronous strobe speed from slow to fast (1HZ~25H

	5
	Golden light 1
Golden light 2
Golden light 3 Dyeing total dimming
Dyeing stroboscopic
	0-255
	Linear dimming from dark to light

	6
	
	0-255
	Linear dimming from dark to light

	7
	
	0-255
	Linear dimming from dark to light

	8
	
	0-255
	Linear dimming from dark to light

	9
	
	0
	No function

	
	
	1-255
	Synchronous strobe speed from slow to fast (1HZ~25H

	10
11
12
13
14
15
16
17
18
19
20
21
22
	ight 1 (dyeing effect runni ight 1 (dyeing effect backg Dyed blue light 1
Dyed red light 2 Dyed green light 2 Dyed blue light 2 Dyed red light 3 Dyed green light 3 Dyed blue light 3 Beam red light Beam green light Blue light beam
Beam white light
	0-255
	Linear dimming from dark to light

	
	
	0-255
	Linear dimming from dark to light

	
	
	0-255
	Linear dimming from dark to light

	
	
	0-255
	Linear dimming from dark to light

	
	
	0-255
	Linear dimming from dark to light

	
	
	0-255
	Linear dimming from dark to light

	
	
	0-255
	Linear dimming from dark to light

	
	
	0-255
	Linear dimming from dark to light

	
	
	0-255
	Linear dimming from dark to light

	
	
	0-255
	Linear dimming from dark to light

	
	
	0-255
	Linear dimming from dark to light

	
	
	0-255
	Linear dimming from dark to light

	
	
	0-255
	Linear dimming from dark to light

	
23
	
golden light) macro functio
	0-4
	neutrality

	
	
	5-85
86-170
171-255
	Built-in effect 1 (from slow to fast)
Built-in effect 2 (from slow to fast) Built-in effect 3 (from slow to fast)

	
	
	
	

	

24
	

dyeing light) macro functio
	0-4
	neutrality

	
	
	4-45
	Built-in effect 1 (from slow to fast)

	
	
	46-87
	Built-in effect 2 (from slow to fast)

	
	
	88-129
	Built-in effect 3 (from slow to fast)

	
	
	130-171
	Built-in effect 4 (from slow to fast)

	
	
	172-213
	Built-in effect 5 (from slow to fast)

	
	
	213-255
	Built-in effect 6 (from slow to fast)

	
25
	
(beam) macro function
	0-4
	neutrality

	
	
	5-85
86-170
171-255
	Built-in effect 1 (from slow to fast) Built-in effect 2 (from slow to fast)
Built-in effect 3 (from slow to fast)

	
	
	
	

	26	reset
	0-199
200-255
	neutrality
reset



	serial number
	English
display
	explain

	1
	ADDR
	A001---A512 address code

	2
	MANU
	Operation mode selection

	3
	RUN
	control)

	4
	CHND
	15CH, 20CH and 26CH channel selection

	5
	SOUD
	ON, OFF sound control switch

	6
	LED
	ON, OFF background light switch

	7
	DISP
	YES, NO reverse display

	8
	PSET
	YES, NO motor x reverse

	9
	TILT
	YES, NO motor y reverse

	10
	VER
	V101 software version number

	11
	FAET
	YES, NO restore factory settings.



image1.png




